Global Security Requirements

# Revision

Version 3

11/15/21 10:01 AM

# SME

Charles Wilson

# Abstract

This document describes the process for creation of a set of security requirements to be used across all products.

# Group / Owner

security / Systems Requirements Planner

# Motivation

This document is motivated by the need to have formal processes in place for the creation of security requirements for the development of safety-critical, cyber-physical systems for certification of compliance to standards such as **ISO 21434** and **ISO 26262**.

# License

This work was created by **Motional** and is licensed under the **Creative Commons Attribution-Share Alike (CC4-SA)** License.

[**https://creativecommons.org/licenses/by/4.0/legalcode**](https://creativecommons.org/licenses/by/4.0/legalcode)

# Overview

In order to create a system with the complexity of an autonomous vehicle, it is necessary to first create a uniformly applicable set of security requirements. This is especially important given that an autonomous vehicle is a safety-critical cyber-physical system.

# Process

The global set of security requirements will be created through the application of gap analysis using a security requirements taxonomy [**[1]**](#ref_01). These requirements will then be entered into the requirements tracking system. There they will be tagged based on their **AVCDL** phase of use. They will then be normalized to INCOSE standards using a requirements analysis tool.

# References

1. **Security Requirements Taxonomy**